> # IP Services

> # IP Routes

> Field | Description
> --- | ---
> Routing Enabled | When this check box is enabled, the switch is acting as in IP router.
> Destination, Mask, Gateway | The value that identifies the local interface through which the next hop of this route should be reached.
> Metric | The primary routing metric for this route.
> Interface | The local interface through which the next hop of this route should be reached.
> Active | Indicates whether the route is active.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.