> # Port Security Config Database

> Field | Description
> --- | ---
> Interface or fWWN | Represents the address of the port on the local device through which the device specified can FLOGI. If fwwn, then the value is the fabric WWN of a port on the local device. If intfIndex, then a port on the local device is being represented by its interface. If wildCard, then it represents a wild-card entry. The wild-card represents any port on the local device.
> Type | The mechanism to identify a switch port.
> WWN | Represents the logging-in device address.
> Available Interface | Displays the available interface. The interfaces available are: Fibre Channel PortChannel Ethernet PortChannel VFC

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.