> # Configuring an iSCSI RADIUS Server

> ## Detailed Steps

> To configure an iSCSI RADIUS server, follow these steps:

> 1. Configure the RADIUS server to allow access from the Cisco MDS switch's management Ethernet IP address.
> 2. Configure the shared secret for the RADIUS server to authenticate the Cisco MDS switch.
> 3. Configure the iSCSI users and passwords on the RADIUS server.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.