Enabling Clustering Using DCNM-SAN

Note All the MDS switches with SME interfaces in the cluster should match the authentication credentials used by DCNM-SAN.

Detailed Steps

To enable clustering using DCNM-SAN, follow these steps:

1. In the Physical Attributes pane, select Intelligent Features > SME > Clusters.

2. From the Control tab in the information pane, locate the switch.

3. From the drop-down menu in the Command column, select enable. The default is noSelection.

Note You can select enable on multiple switches, and then click Apply.

4. Click Apply.