> # FC Interface Monitor Class 2 Traffic

> The Monitor dialog boxes have special Monitor Dialog Controls.

> Field | Description
> --- | ---
> In Octets/In Frames | The number of Class 2 frame bytes and frames, including the frame delimiters, received by this port from its attached Nx_Port.
> Out Octets/Out Frames | The number of Class 2 frame bytes and frames, including the frame delimiters, delivered through this port to its attached Nx_Port.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.