> # Enabling Contiguous Domain ID Assignments

> ## Detailed Steps

> To enable contiguous domains in a specific VSAN (or a range of VSANs), follow these steps:

> 1. Expand Fabric > All VSANs and then select Domain Manager in the Logical Domains pane for the fabric and VSAN that you want to enable contiguous domains for.

> You see the running configuration of the domain in the Information pane.

> 2. Click the Configuration tab and check the Contiguous Allocation check box for each switch in the fabric that will have contiguous allocation.
> 3. Click the Apply Changes icon to save these changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.