> # DPVM Configuration Guidelines

> When NPV is enabled, the following requirements must be met before you configure DPVM on the NPV core switch:

> - You must explicitly configure the WWN of the internal FLOGI in DPVM. If DPVM is configured on the NPV core switch for an end device that is connected to the NPV device, then that end device must be configured to be in the same VSAN. Logins from a device connected to an NPV device will fail if the device is configured to be in a different VSAN. To avoid VSAN mismatches, ensure that the internal FLOGI VSAN matches the port VSAN of the NP port.
> - The first login from an NP port determines the VSAN of that port. If DPVM is configured for this first login, which is the internal login of the NPV device, then the NPV core switch’s VSAN F port is located in that VSAN. Otherwise, the port VSAN remains unchanged.

> For details about DPVM configuration, see the Cisco MDS 9000 Family NX-OS Fabric Configuration Guide.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.