> # FCC

> Field | Description
> --- | ---
> Enable | Enable Fabric Congestion Control
> Priority | Specifies the priority level for the frames.
> EdgeQuenchPktsRecd | The number of Edge Quench packets received and processed on this port.
> EdgeQuenchPktsSent | The number of Edge Quench packets generated on this Port as result of congestion.
> PathQuenchPktsRecd | The number of Path Quench packets received and processed on this port.
> PathQuenchPktsSent | The number of Path Quench packets generated on this Port as result of congestion.
> CurrentCongestionState | The current FCC congestion state of this Port indicating the severity of the congestion.
> LastCongestedTime | When the congestion state of the Port changed to noCongestion from some other value. N/A if the congestion state of the Port has never transitioned to noCongestion since the last restart of the device.
> LastCongestionStartTime | When the congestion state of the port changed from noCongestion to some other value.
> IsRateLimitingApplied | If true, rate limiting is currently being applied on this port.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.