## Viewing Events Registration

To enable Send Syslog, Send Traps and Delayed Traps you need to configure the following in the DCNM-SAN client:

• Enabling Send Syslog - Log into the DCNM-SAN client. In the Physical Attributes pane, Select Events>Syslog>Servers. Click the Create Row icon, provide the required details and click Create.

• Enabling Send Traps - Log into the DCNM-SAN client. In the Physical Attributes pane, Select Events>SNMP Traps>Destination. Click the Create Row icon, provide the required details and click Create.

• Enabling Delayed Traps - Log into the DCNM-SAN client. In the Physical Attributes pane, Select Events>SNMP Traps>Delayed Traps. In the Feature Enable column, use the checkboxes to enable delayed traps for the switch and specify the delay in minutes.

1. From the menu bar, choose Admin > Events > Registration.

The SNMP and Syslog receivers along with the statistics information are displayed.

2. Select Enable Syslog Receiver checkbox and click Apply to enable the syslog receiver if it is disabled in the server property.

To configure the Event Registration/Syslog properties, select Admin>Server Properties and follow the on-screen instructions.

3. Select Copy Syslog Messages to DB and click Apply to copy the syslog messages to the database. If this option is not select, the events will not be displayed in the events page of the Web client.

4. The columns in the second table displays the following:

• Switches sending traps

• Switches sending syslog

• Switches sending syslog accounting

• Switches sending delayed traps