> # Virtual FC Interfaces

> The following fields in the table can be modified: Description, Bind Type, Bind Interface, Bind MAC Address, FCF Priority, VSAN ID Port, Mode Admin, Status Admin. The remaining fields are for information only.

> Field | Description
> --- | ---
> Switch | Name of the switch hosting this interface.
> Interface | Interface name.
> Description | Text description of the interface as specified by a network manager.
> VIG Id | Virtual interface group to which this virtual FC interface is bound.
> Bind Type | The type of interface associated with this virtual FC interface - physical Ethernet interface or MAC address of the FCoE Node (ENode).
> Bind Interface | Physical Ethernet interface or Ethernet port channel associated with this virtual FC interface.
> Bind MACAddress | MAC address of an FCoE Node (ENode) or a remote Fibre Channel Forwarder (FCF) identified by the virtual FC interface.
> FCF Priority | The FCoE Initialization Protocol (FIP) priority value advertised by the FCF to ENodes.
> VSAN ID Port | VSAN ID to which this interface is statically assigned.
> VSAN Id Dynamic | Index of the VSAN to which this interface is statically assigned.
> Mode Admin | The port mode configured by the user. Virtual FC interfaces support only fabric port (F Port) mode.
> Rate Mode | Specifies the interface as dedicated mode or shared mode.
> Speed Oper | Operational speed.
> Mode Oper | The current operating mode of the port.
> Speed Admin | The port speed configured by the user.
> Status Service | Specifies whether the interface is in service or out of service.
> Status Admin | The desired state of the interface.
> Status Oper | The current operational state of the interface.
> Status FailureCause | The cause of current operational state of the port.
> Status LastChange | When the interface entered its current operational state. If the current state was entered prior to the last re-initialization of the local network management subsystem, then this value is N/A.

> Note VIG Id field applies only to N5k switches running version less than 4.0(1a).

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.