> # Transitioning from IPv4 to IPv6

> Cisco MDS NX-OS does not support any transitioning mechanisms from IPv4 to IPv6. However, you can use the transitioning schemes in the Cisco router products for this purpose. For information on configuring Cisco routers to transition your network, refer to the “Implementing Tunneling for IPv6” chapter in the Cisco IOS IPv6 Configuration Guide.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.