> # FCIP FICON Configuration

> Field | Description
> --- | ---
> Interface | This is a unique value that identifies the interface on this FCIP device to which this link pertains.
> VSAN List Admin | This is the list of VSANs (in the range 1 through 2047) for which Ficon Tape Acceleration is configured. Only VSANs with a cficonVsanEntry of CISCO-FICON-MIB present can be configured for Ficon Tape Acceleration.
> VSAN List Oper | This is the list of VSANs (in the range 1 through 2047) for which Ficon Tape Acceleration is operationally "ON".

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.