> # Assigning VSAN Membership for iSLB Initiators

> Individual iSLB hosts can be configured to be in a specific VSAN (similar to the DPVM feature for Fibre Channel). The specified VSAN overrides the iSCSI interface VSAN membership.

> For more information, see the Fabric Configuration Guide, Cisco DCNM for SAN.

> Note Specifying the iSLB initiator VSAN is the same as for an iSCSI initiator. See the "VSAN Membership for iSCSI" procedure.

> Note When an iSLB initiator is configured in any other VSAN (other than VSAN 1, the default VSAN), for example VSAN 2, the initiator is automatically removed from VSAN 1. If you also want it to be present in VSAN 1, you must explicitly configure the initiator in VSAN 1.

> See the "Configuring iSLB Using Device Manager" procedure.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.