## Selecting the Key Manager and SSL Settings

1. From the menu bar, select Config>Provision.

The Key Manager Settings window is displayed with the following options:

• None-No Key Manager selected for SME.

• Cisco-Cisco Key Manager selected for SME.

• RSA-RSA Key Manager selected for SME

Note Once you have selected a Key Manager, you will not be able to change it.

1. Select one of the Radio buttons and click Submit Settings.

The Key Manager Settings window is displayed.

The KMC SSL Settings pane displays the location where the certificate is stored.

2. If you want to edit the SSL Settings, click Edit SSL Settings.

3. Use the drop-down to select the SME KMC Trust Certificate.

4. Use the drop-down to select the SME KMC Server Certificate.

5. Specify and confirm the Server Cert Password.

6. Click Submit SSL Settings.

7. In the High Availability Settings pane, click Edit HA Settings to specify the KMC Role of this Server and SME Secondary Server Address.

8. Click Submit HA Settings to confirm.