> # Default Settings

> Table 25-3 lists the default settings for FICON features.

> Table 25-3 Default FICON Settings
> Parameters | Default
> --- | ---
> FICON feature | Disabled.
> Port numbers | Same as port addresses.
> FC ID last byte value | 0 (zero).
> EBCDIC format option | US-Canada.
> Switch offline state | Hosts are allowed to move the switch to an offline state.
> Mainframe users | Allowed to configure FICON parameters on Cisco MDS switches.
> Clock in each VSAN | Same as the switch hardware clock.
> Host clock control | Allows host to set the clock on this switch.
> SNMP users | Configure FICON parameters.
> Port address | Not blocked.
> Prohibited ports | Ports 90–253 and 255 for the Cisco MDS 9200 Series switches. Ports 250–253 and 255 for the Cisco MDS 9500 Series switches.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.