> # Supported Hardware

> You can configure the FCIP and iSCSI features using one or more of the following hardware:

> - IPS-4 and IPS-8 modules (refer to the Cisco MDS 9200 Series Hardware Installation Guide or the Cisco MDS 9500 Series Hardware Installation Guide for more information)
> - MPS-14/2 module (refer to the Cisco MDS 9200 Series Hardware Installation Guide or the Cisco MDS 9500 Series Hardware Installation Guide for more information).

> Note In both the MPS-14/2 module and the Cisco MDS 9216i integrated supervisor module, the port numbering differs for the Fibre Channel ports and the Gigabit Ethernet ports. The Fibre Channel ports are numbered from 1 through 14 and the Gigabit Ethernet ports are numbered 1 and 2.

> - Cisco MDS 9216i Switch (refer to the Cisco MDS 9200 Series Hardware Installation Guide).

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.