> # Power Supplies

> Field | Description
> --- | ---
> Name | Power supply location.
> TotalPowerAvailable | Shows the available power. In combined mode, the total available power is twice the lesser of the two power supplies.
> Redundant/Combined | Select to determine how the power supplies are configured. Redundant mode provides a backup power supply if one should fail, but the total power available is less.
> ModelName | The model identifier.
> OperStatus | Operational power state.
> TotalAvailable | Total power available for power supply usage. When Mode is redundant, the total power available will be the lesser power capacity of the power supplies. When Mode is combined, the total power available will be twice the lesser of the power capacities of the operating power supplies.
> TotalReserved | Total current drawn by powered-on FRUs

> Note If the power supply to the Uros and Paradise is either interrupted or turned off, the OperStatus in the power supply table displays "offEnvOther". However, the corresponding entry for the powered down device the inventory table will remain.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.