> # Configuring Autonegotiation

> By default, autonegotiation is enabled all Gigabit Ethernet interface. You can enable or disable autonegotiation for a specified Gigabit Ethernet interface. When autonegotiation is enabled, the port automatically detects the speed or pause method, and duplex of incoming signals based on the link partner. You can also detect link up conditions using the autonegotiation feature.

> ## Detailed Steps

> To configure autonegotiation, follow these steps:

> 1. Expand Switches > Interfaces > Ethernet > IPS.

> You see the Gigabit Ethernet Configuration in the Information pane.

> 2. In the General tab, you can enable or disable the Auto Negotiate option for a specific switch.
> 3. Click Apply Changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.