> # FCIP Interfaces Interfaces

> Field | Description
> --- | ---
> Description | Alias name for the interface as specified by a network manager.
> PortVsan | The VSAN ID to which this interface is statically assigned.
> Oper | The current operating mode of the port.
> AutoChannelCreate | If checked, automatically create the PortChannel.
> Admin | The desired state of the interface.
> Oper | The current operational state of the interface.
> FailureCause | The cause of current operational state of the port.
> LastChange | When the interface entered its current operational state. If the current state was entered prior to the last re-initialization of the local network management subsystem, then this value is N/A.
> FICON Address | The FICON port address of this port.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.