> # IKE Initiator Version

> Field | Description
> --- | ---
> Address | The address of the remote peer corresponding to this conceptual row. This object cannot be modified while the corresponding value of cicIkeCfgInitiatorStatus is equal to active.
> Version | The IKE protocol version used when connecting to a remote peer specified in cicIkeCfgInitiatorPAddr. This object cannot be modified while the corresponding value of cicIkeCfgInitiatorStatus is equal to active.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.