Adding Tape Paths

Use the Tape Path Wizard to quickly add or modify tape paths between hosts and target backup devices.

Detailed Steps

To add a tape path to a tape device, follow these steps:

1. Select a tape device.

2. Click Add.

3. Select the appropriate fabric and enter the VSAN, initiator and target WWNs, and the LUN. Click Next.

4. Confirm the addition of the new tape path. Click Confirm to close the SME wizard and to return to the DCNM-SAN SME screen.