> # Bandwidth Reservation: 24-Port 48-Gbps Fibre Channel module

> RateMode Config Macro | Description
> --- | ---
> Dedicated 8 Gbps on the first port of each group and the remaining ports 8G shared | Allocates a rate mode and admin speed of 8Gbps on the first port of each group and the remaining ports share 8 Gbps depending on the operational speed of the ports
> Shared Auto on all ports (initial & default settings) | Allocates a rate mode and admin speed of 8 Gbps on all the available ports. This is the default setting.

> #

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.