> # Advanced VSAN Membership for iSCSI Hosts

> An iSCSI host can be a member of multiple VSANs. In this case, multiple virtual Fibre Channel hosts are created, one in each VSAN in which the iSCSI host is a member. This configuration is useful when certain resources such as Fibre Channel tape devices need to be shared among different VSANs.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.