> # FC Interface Monitor Protocol

> The Monitor dialog boxes have special Monitor Dialog Controls.

> Field | Description
> --- | ---
> LRRIn | The number of Link reset responses received by the FC-port.
> LRROut | The number of Link reset responses transmitted by the FC-port.
> OlsIns | The number of Offline Sequence errors received by the FC-Port.
> OlsOuts | The number of Offline Sequence errors issued by the FC-Port.
> NOSIn | The number of Non-Operational Sequences received by the FC-port.
> NOSOut | The number of Non-Operational Sequences transmitted by the FC-port.
> LinkResetIns | The number of link reset protocol errors received by the FC-Port from the attached FC-port.
> LinkResetOuts | The number of link reset protocol errors issued by the FC-Port to the attached FC-Port.
> TxWaitCount | The number of times the FC-port waited due to lack of transmit credits.
> RxBBCredit | The maximum number of receive buffers available for holding Class 2, Class 3 received from the logged-in Nx_Port. It is for buffer-to-buffer flow control in the incoming direction from the logged-in Nx_Port to FC-port.
> TxBBCredit | The total number of buffers available for holding Class 2, Class 3 frames to be transmitted to the logged-in Nx_Port. It is for buffer-to-buffer flow control in the direction from FC-Port to Nx_Port.
> BBCreditTransitionFromZe ro | The number of transitions of BB credit out of zero state.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.