> # Moving a Feature to a Different Region

> ## Prerequisites

> Before moving a feature to a new region, create the new region in the All Regions tab. That is, a new row has to be added in the All Regions tab with the new Region ID.

> ## Detailed Steps

> To move a feature to a different region, follow these steps:

> 1. Expand Switches and select CFS from the Physical Attributes pane.

> The information pane displays the Global, IP Multicast, Feature by Region, and All Regions tabs.

> 2. Click the Feature by Region tab.
> 3. Double-click the RegionId cell in the required row.

> The cursor blinks in the cell prompting a change in the value.

> 4. Change the RegionId value to the required region.
> 5. Click the Apply Changes button on the tool bar to commit the change.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.