> # Configuring RMON Alerts

> ## Detailed Steps

> To configure RMON alert groups, follow these steps:

> 1. Select a switch in the Fabric pane.
> 2. Expand Events and select Call Home in the Physical Attributes pane.

> You see the Call Home information in the Information pane.

> 3. Click the Profiles tab.

> You see the Call Home profiles.

> 4. Select the Create Row icon.

> You see the Create Call Home Profile dialog box.

> 5. Select switches to send alerts.
> 6. Enter the name of the profile.
> 7. Select the message format, message size, and message severity level.
> 8. Check the RMON check box in the AlertGroups section.
> 9. Click Create to create the profile for the RMON-based alerts.
> 10. Close the dialog box.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.