> # Bandwidth Reservation: 32-Port 256-Gbps Fibre Channel module

> RateMode Config Macro | Description
> --- | ---
> Dedicated 8 Gbps on on all ports | Allocates a rate mode and admin speed of 8 Gbps on all the available ports.
> Shared 8 Gbps on on all ports — initial and default settings. | Allocates a rate mode and admin speed of shared 8 Gbps on all the available ports.
> Dedicated 10G on following ports: 2,3,4,5,6,8 (ports 1 and 7 disabled) 10,11,12,13,14,16 (ports 9 and 15 disabled) 18,19,20,21,22,24 (ports 17 and 23 disabled) 26,27,28,29,30,32 (ports 25 and 31 disabled) | Allocates a rate mode and admin speed of 10Gbps on the specified ports.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.