> # Assigning a Port Address Name

> Note To view the latest FICON information, you must click the Refresh button. See the "Automatically Saving the Running Configuration" topic.

> ## Detailed Steps

> To assign a port address name in Device Manager, follow these steps:

> 1. Choose FICON > VSANs.
> 2. Select a VSAN ID and click Port Configuration.

> You see the FICON Port Configuration dialog box.

> 3. Enter the Port Configuration information.
> 4. Click Apply to save the configuration information.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.