> # FC Interface Monitor Traffic

> The Monitor dialog boxes have special Monitor Dialog Controls.

> Field | Description
> --- | ---
> C3 Rx Bytes | The number of Class 3 bytes, including the frame delimiters, received by this port from its attached Nx_Port.
> C3 Rx Frames | The number of Class 3 frames, including the frame delimiters, received by this port from its attached Nx_Port.
> C3 Tx Bytes | The number of Class 3 bytes, including the frame delimiters, transmitted by this port to its attached Nx_Port.
> C3 Tx Frames | The number of Class 3 frames, including the frame delimiters, transmitted by this port to its attached Nx_Port.
> CF Rx Bytes | The number of Class F bytes, including the frame delimiters, received by this port from its attached Nx_Port.
> CF Rx Frames | The number of Class F frames, including the frame delimiters, received by this port from its attached Nx_Port.
> CF Tx Bytes | The number of Class F bytes, including the frame delimiters, transmitted by this port to its a attached Nx_Port.
> CF Tx Frames | The number of Class F frames, including the frame delimiters, transmitted by this port to its attached Nx_Port.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.