Topology

This displays the current physical topology with color- coding (displayed with a key in the lower right corner) for ISL utilization. You can hover over the switch indication circles to display the configured switch name, model, IP address, SW version, bandwidth utilized and the CPU and memory percentage.

You can choose the Layout icon and to select layout display. There are three option:

• Organic Layout

• Radial layout

• Circular Layout

You can use the checkboxes to select the Channel Member, NPV and FEX.

Use the +/- icons at the bottom right of the screen to maximize/minimize the topology view.

Click the Filter on VSAN/VLAN name or id icon to filter the view.

Click the Show Overview icon to view a miniature view of the topology and then click-drag around that area to move the main view.

You can use the Save, Restore or Clear layout icon to save, restore or clear the layout for the selected scope.