> # Port Administrative Speeds

> By default, the port administrative speed for an interface is automatically calculated by the switch.

> For internal ports on the Cisco Fabric Switch for HP c_Class BladeSystem and Cisco Fabric Switch for IBM BladeCenter, a port speed of 1 Gbps is not supported. Auto-negotiation is supported between 2 Gbps and 4 Gbps only. Also, if the BladeCenter is a T chassis, then port speeds are fixed at 2 Gbps and auto-negotiation is not enabled.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.