> # Launching Call Home Wizard

> ## Before You Begin

> - Enable the global CFS on the switch from DCNM-SAN configuration table.
> - Clear the CFS lock on the switch.
> - Check the merger status of CFS on the switch. If a merger failure is found, the wizard clears up the merge failure in the backend process while running the wizard.

> ## Detailed Steps

> To configure Call Home wizard, follow these steps:

> 1. Select a fabric in the logical domain tree.
> 2. Select Tools, Events and Call Home.

> The master switch pane is displayed.

> 3. (Optional) You can also launch the Call Home wizard by clicking the CallHome Wizard icon in the Call Home Control tab.
> 4. Select a Master Switch and click Next.

> The contact information pane is displayed.

> 5. Enter the Contact, Phone Number, Email Address and the Street Address information.

> Note You must specify all of the four parameters before clicking Next.

> 1. Click Next.

> The Email Setup pane is displayed.

> 2. In the Email SMTP Servers tab, enter the Primary SNTP Server address.

> You can specify up to two SMTP servers if the master switch is version 5.0 or above. However, you cannot specify a secondary SMTP server if the master switch version is below 5.0.

> The wizard creates new rows in the SMTP server table.

> 3. In the Destination tab, click Add to enter the Call Home destinations.

> You can enter up to three Call Home destinations.

> 4. (Optional) Click Remove to delete a Call Home destination entry.
> 5. From the drop-down list, select Protocol and Profile.

> The Profile drop-down lists three default profiles: xml, short_txt and full_txt.

> 6. Click Finish to configure the wizard.

> The Status Dialog window is displayed.

> All major configuration steps and failures are displayed in the Status Dialog window.

> 7. Click Run Test to perform the Call Home test.
> 8. Click Yes to test the command on all switches in the selected fabric or click No to close the window.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.