> # Reading the IP-ACL Log Dump

> Use the LogEnabled check box option during IP filter creation to log information about packets that match this filter. The log output displays the ACL number, permit or deny status, and port information.

> For the input ACL, the log displays the raw MAC information. The keyword “MAC=” does not refer to showing an Ethernet MAC frame with MAC address information. It refers to the Layer 2 MAC-layer information dumped to the log. For the output ACL, the raw Layer 2 information is not logged.

> The following example is an input ACL log dump:

>     Jul 17 20:38:44 excal-2
>     %KERN-7-SYSTEM_MSG:
>     %IPACL-7-DENY:IN=vsan1 OUT=
>     MAC=10:00:00:05:30:00:47:df:10:00:00:05:30:00:8a:1f:aa:aa:03:00:00:00:08:00:45:00:00:54:00
>     :00:40:00:40:01:0e:86:0b:0b:0b:0c:0b:0b:0b:02:08:00:ff:9c:01:15:05:00:6f:09:17:3f:80:02:01
>     :00:08:09:0a:0b:0c:0d:0e:0f:10:11:12:13:14:15:16:17:18:19:1a:1b:1c:1d:1e:1f:20:21:22:23:24
>     :25:26:27:28:29:2a:2b SRC=11.11.11.12 DST=11.11.11.2 LEN=84 TOS=0x00 PREC=0x00 TTL=64 ID=0
>     DF PROTO=ICMP TYPE=8 CODE=0 ID=277 SEQ=1280

> The following example is an output ACL log dump:

>     Jul 17 20:38:44 excal-2
>     %KERN-7-SYSTEM_MSG:
>     %IPACL-7-DENY:IN= OUT=vsan1 SRC=11.11.11.2 DST=11.11.11.12 LEN=84 TOS=0x00 PREC=0x00
>     TTL=255 ID=38095 PROTO=ICMP TYPE=0 CODE=0 ID=277 SEQ=1280

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.