> # Cisco DCNM-SAN Client Quick Tour: Admin Perspective

> This section describes the Cisco DCNM-SAN Client interface shown in Figure 5-1.

> Figure 5-1 Cisco DCNM-SAN Main Window

> 1 | Menu bar—Provides access to options that are organized by menus.
> 2 | Toolbar—Provides icons for direct access to the most commonly used options on the File, Tools, and Help menus.
> 3 | Information pane—Displays information about whatever option is selected in the menu tree.
> 4 | Status Bar (right side)—Shows the last entry displayed by the discovery process and the possible error message.
> 5 | Fabric pane—Displays a map of the network fabric, including switches, hosts, and storage. It also provides tabs for displaying log and event data.
> 6 | Status Bar (left side)—Shows short-term transient messages, such as the number of rows displayed in a table.
> 7 | Physical Attributes pane—Displays a tree of available configuration tasks depending on the fabric, VSAN, or zone selected previously. Lists the switches and end devices in the logical selection.
> 8 | Logical Domains pane—Displays a tree of configured SAN, fabrics, VSANs, and zones, and provides access to user-defined groups. The label next to the segmented VSAN indicates the number of segments.

> Note You can resize each pane by dragging the boundaries between each region or by clicking the Minimize or Maximize controls.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.