> # FC Interfaces FLOGI

> Field | Description
> --- | ---
> FcId | The address identifier that has been assigned to the logged-in Nx_Port.
> PortName | The world wide name of the logged-in Nx_Port.
> NodeName | The world wide name of the Remote Node the logged-in Nx_Port belongs to.
> Original PWWN | The original port WWN for this interface
> Version | The version of FC-PH that the Fx_Port has agreed to support from the Fabric Login.
> BBCredit Rx | The maximum number of receive buffers available for holding Class 2, Class 3 received from the logged-in Nx_Port. It is for buffer-to-buffer flow control in the incoming direction from the logged-in Nx_Port to FC-port.
> BBCredit Tx | The total number of buffers available for holding Class 2, Class 3 frames to be transmitted to the logged-in Nx_Port. It is for buffer-to-buffer flow control in the direction from FC-Port to Nx_Port. The buffer-to-buffer flow control mechanism is indicated in the respective BbCreditModel.
> CoS | The classes of services that the logged-in Nx_Port has requested the FC-Port to support and the FC-Port has granted the request.
> Class2 RxDataSize | The Class 2 Receive Data Field Size of the logged-in Nx_Port. Specifies the largest Data Field Size for an FT_1 frame that can be received by the Nx_Port.
> Class2 SeqDeliv | Whether the FC-Port has agreed to support Class 2 sequential delivery during the Fabric Login. This is meaningful only if Class 2 service has been agreed. This is applicable only to Fx_Ports.
> Class3 RxDataSize | The Class3 Receive Data Field Size of the logged-in Nx_Port. Specifies the largest Data Field Size for an FT_1 frame that can be received by the Nx_Port.
> Class3 SeqDeliv | Whether the FxPort has agreed to support Class 3 sequential delivery during the Fabric Login. This is meaningful only if Class 3 service has been agreed. This is applicable only to Fx_Ports.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.