## Enabling SME Services

To enable SME services, do the following tasks:

• Enable clustering on all the SME switches. For more information, refer to the “Enabling Clustering Using DCNM-SAN” section on page 2-17.

• Enable SME services using either DCNM-SAN or Device Manager. For more information, refer to the “Enabling SME” section on page 2-18.

• Set the FC-Redirect version to 2 (if you are using SAN-OS Release 3.1(1a) or later or NX-OS Release 4.x).