> # Call Home Profiles

> Field | Description
> --- | ---
> MsgFormat | XML, full text, or short text.
> MaxMsgSize | Maximum message size that can be sent to destination pointed to by this destination profile.
> MsgLevel | Threshold level, used for filtering alert messages sent to a destination. Callhome alert message with severity level lower than the configured threshold level would not be sent. The default threshold level is debug (1), which means all the alert messages will be sent.
> AlertGroups | The list of configured alert groups for this destination profile.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.