> # RLIR ERL

> Field | Description
> --- | ---
> Vsan ID | VSAN Identifier of the port.
> FC ID | Fibre Channel identifier of the subscribing Nx_Port.
> Format | The device type for which the Nx_Port receives RLIR ELS."
> RegType | The subscriber’s registration type. ConditionalRx - The Nx_Port will be the recipient of a link incident record only if no other recipients from the ERL on the VSAN is chosen. AlwaysRx - The Nx_Port will be always chosen as the recipient of a link incident records.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.