> # Configuring FCoE Using Device Manager

> ## Detailed Steps

> To configure FCoE on a switch using Device Manager, follow these steps:

> 1. Launch Device Manager from the Cisco Nexus 5000 Series switch.
> 2. Choose FCoE > Config.

> You see the FCoE Config dialog box.

> The Config tab displays the FCoE parameters, such as FC Map, default FCF priority value, and FKA advertisement period, for each Cisco Nexus 5000 Series switch that runs Cisco NX-OS Release 4.1(3) or later releases. Table 18-1 lists the FCoE parameters for a switch.

> 3. Double-click the relevant FCoE parameter for a switch, and modify the value of the parameter.
> 4. Click Apply to save the changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.