> # FL Port

> In fabric loop port (FL port) mode, an interface functions as a fabric loop port. This port may be connected to one or more NL ports (including FL ports in other switches) to form a public arbitrated loop. If more than one FL port is detected on the arbitrated loop during initialization, only one FL port becomes operational and the other FL ports enter nonparticipating mode. FL ports support class 2 and class 3 service.

> Note FL port mode is not supported on 4-port 10-Gbps switching module interfaces.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.