> # FlexAttach Virtual pWWN CFS Distribution

> The FlexAttach virtual pWWN configuration is distributed for CFS through IPv4, and is enabled by default. The FlexAttach virtual pWWN distribution, by default, is on CFS region 201. The CFS region 201 links only to the NPV-enabled switches. Other CFS features such as syslog is on region 0. Region 0 will be linked through IPv4 for all NPV switches on the same physical fabric. If CFS has an option to link through IPv4 or ISL, then CFS will select the ISL path.

> Note NPV switches do not have ISL (E or TE ports) and are linked through IPv4.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.