> # Zoneset Active Zones Attributes

> Field | Description
> --- | ---
> Name | Zone name.
> Read Only | Indicates if only SCSI read operations are allowed on members of the default zone which are SCSI targets on this VSAN. If true, then only SCSI read operations are permitted. So, this default zone becomes a read-only default zone on this VSAN. If false, then both SCSI read and write operations are permitted.
> QoS | Specifies whether the QoS attribute for the default zone on this VSAN is enabled. If true, then QoS attribute for the default zone on this VSAN is enabled. If false, then the QoS attribute for the default zone on this VSAN is disabled.
> QoS Priority | Specifies QoS priority value (Low, Medium, or High).
> Broadcast | Specifies if broadcast zoning is enabled on this default zone on this VSAN. If true, then it is enabled. If false, then it is disabled.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.