> # Quick Configuration Tool

> Field | Description
> --- | ---
> Show All Interfaces | Check this checkbox to show all the available interfaces including the interfaces that are not available for binding to a vFC.
> Auto Assigin vFC Id | Check this checkbox to select vFC Id automatically. If you do not select this option you must manually enter a valid vFC Id.
> Switch Operational Type | Click Ethernet Switch if you are not configuring any Fibre Channel interfaces on the switch. Click FCoE Switch if you are configuring Fibre Channel and FCoE interfaces.
> Interface | Name of the physical Ethernet interface. If you hover the cursor over a physical Ethernet interface, any associated virtual interfaces are displayed in the tooltip.
> FCoE VLAN(VSAN) | FCoE VLAN (VSAN) mapping to be used by the interface.
> Admin Mode | Admin mode of the vFC interface, i.e. F or E
> Eth Only | Configures the physical Ethernet without any virtual interfaces. Click the Eth Only button in the column header to set all the interfaces to this value.
> vEth Only | Configures the physical Ethernet to have an associated VIG and a virtual Ethernet interface. Click the vEth Only button in the column header to set all the interfaces to this value.
> vFC Only | Configures the physical Ethernet to have an associated VIG and a virtual FC interface. Click the vFC Only button in the column header to set all the interfaces to this value.
> vFC | Configures the physical Ethernet to have an associated VIG and a virtual FC interface. Click the vFC button in the column header to set all the interfaces to this value.
> vEth + vFC | Configures the physical Ethernet to have an associated VIG, a virtual Ethernet interface and a virtual FC interface. Click the vEth + vFC button in the column header to set all the interfaces to this value.
> Configure Action Status | Displays the current status of the requested configuration changes.

> Note vEth only, vFC only, vEth + vFC columns are not applicable for N5K switches running version 4.0(1a)N1

> Note vFC column is applicable only for N5K switches running version 4.0(1a)N1

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.