# Verifying SME Interface Configuration

To display SME interface configuration information, perform one of the following tasks:

Command | Purpose
show interface sme | Displays the SME interface configuration and statistics.
show int | Displays if the SME interface is down until the interface is added to a cluster.

For detailed information about the fields in the output from these commands, refer to the Cisco MDS 9000 Family NX-OS Command Reference.