> # Security Settings for FlexAttach Virtual pWWN

> Security settings for the FlexAttach virtual pWWN feature are done by port security at the NPV core. Node WWN of the end device is used to provide physical security.

> For more details on enabling port security, refer to the Cisco MDS 9000 Family NX-OS Security Configuration Guide.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.