> # Configuring iSLB Initiator Targets

> You can configure initiator targets using the device alias or the pWWN. You can also optionally specify one or more of the following optional parameters:

> - Secondary pWWN
> - Secondary device alias
> - LUN mapping
> - IQN
> - VSAN identifier

> Note The VSAN identifier is optional if the target is online. If the target is not online, the VSAN identifier is required.

> In addition, you can disable auto-zoning.

> If you configure an IQN for an initiator target, then that name is used to identify the initiator target. Otherwise, a unique IQN is generated for the initiator target.

> ## Detailed Steps

> To configure additional iSLB initiator targets using Device Manager, follow these steps:

> 1. Choose IP > iSCSI iSLB.

> You see the iSCSI iSLB dialog box.

> 2. Click on the initiator you want to add targets to and click Edit Initiator Specific Targets.

> You see the Initiator Specific Target dialog box.

> 3. Click Create to create a new initiator target.

> You see the Create Initiator Specific Target dialog box.

> 4. Fill in the pWWN field with the initiator target pWWN.
> 5. (Optional) Set the Name field to a globally unique identifier (IQN).
> 6. (Optional) Check the NoAutoZoneCreation check box to disable auto-zoning.
> 7. (Optional) Check the TresspassMode check box. See the "LUN Trespass for Storage Port Failover" topic.
> 8. (Optional) Check the RevertToPrimary check box to revert back to the primary port after an HA failover when the primary port comes back up.
> 9. Set the PrimaryVsan to the VSAN for the iSLB initiator target.
> 10. Click Create to create this iSLB initiator target.
> 11. If CFS is enabled, select commit from the CFS drop-down menu.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.