> # Adding an Interface to a PortChannel

> ## Detailed Steps

> Note By default, the CLI adds a interface normally to a PortChannel, while DCNM-SAN adds the interface by force, unless specified explicitly.

> To add an interface or range of interfaces to a PortChannel using DCNM-SAN, follow these steps:

> 1. Expand ISLs and then select Port Channels in the Physical Attributes pane.

> You see the PortChannels in the Information pane.

> 2. Click the Channels tab and find the switch and PortChannel that you want to edit.
> 3. Set Members Admin to the interface or list of interfaces that you want to add to the PortChannel.
> 4. Click the Apply Changes icon to save any modifications or click Undo Changes to discard any changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.