> # Information About FLOGI

> In a Fibre Channel fabric, each host or disk requires an FC ID. If the required device is displayed in the FLOGI table, the fabric login is successful. Examine the FLOGI database on a switch that is directly connected to the host HBA and connected ports. See the "Default Company ID List" topic and the "Switch Interoperability" topic.

> This section includes the following topics:

> - Name Server Proxy
> - About Registering Name Server Proxies
> - About Rejecting Duplicate pWWN
> - About Name Server Database Entries
> - FDMI
> - RSCN
> - About the multi-pid Option
> - RSCN Timer Configuration Distribution Using CFS
> - RSCN Timer Configuration Distribution
> - Locking the Fabric

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.