> # Smart Zoning

> Field | Description
> --- | ---
> Switch | Specifies the type of which where smart zoning feature exists.
> Status | Specifies if the smart zoning feature is enabled or disabled.
> Command | Specifies the switch level command for smart zoning. If the command is disabled in one switch then smart zoning will be disabled in the whole fabric.
> Last Command | Specified the previous command mode of the switch. Enabled or disabled.
> Result | Specifies if the enable or disable action has been successful or unsuccessful.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.