> # Persistent FC IDs

> When persistent FC IDs are enabled, the following consequences apply:

> - The currently in use FC IDs in the fcdomain are saved across reboots.
> - The fcdomain automatically populates the database with dynamic entries that the switch has learned about after a device (host or disk) is plugged into a port interface.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.